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ENEE 302 Possible to do items #6

1. 
Design a 2-input CMOS NAND gate, biased by Vdd and ground, such that if initially both A and B inputs are at 0 and the B input changes to a 1, the output voltage will be Vdd/2 when the B input hits Vdd/2. Check this with Spice. Determine the output voltage for your design when initially A=1, B=0, and B changes to a 1 as it passes through Vdd/2. Also do a set of runs for various PMOS width parameters to see the effect of changing the PMOS widths.    

2. 
Do a similar design as 1. above for a 2-input CMOS NOR gate. 

3. 
Using your CMOS circuit of 2, design a CMOS NOR SR (flip-flop) latch and check its operation in Spice. Repeat by designing a CMOS NAND SR latch. 

