Instructions for the TA:

1. All TA should make sure the students attending the lab are enrolled in the respective sections. 
To check the roaster log onto UMEG.UMD.EDU
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2. Make sure the Probes are at the same compensation 10x or 1x. 
3. Power Supply are Floating. Please establish Ground before any experiment. 
4. In case, students use IC, make sure they use the IC puller.
5. Enforce student to use the FPGA Board, outside the FPGA Box.  
